Description:		Description:	
2 Extractor Spring 		43 Hammer Pin 	
3 Plunger 		44 R Sear 	
4 R-Extractor 		45 Pin For Safety and 
 Trumb Piece 	
5 L-Extractor 		46 Thumb Piece 	
6 Screw 		47 Locking Bolt 	
7 Pin 		48 Connecting Rod 	
11 Front Sight 		49 Locking Bolt Spring 	
12 Forend 		50 Cam Stop 	
13 Washer 		51 Threaded Connecting Piece 	
14 Spring 		52 Locking Bolt Lever 	
15 Latch Bdy		53 Ball 	
16 Forend Latch		54 Sear Lifter Lever Spring 	
17 Pin 		55 Safety 	
18 Screw 
19 Screw 
20 Screw 		56 Sear Lifter Lever 	
21 Lever Pin 		57 Sear Lifter 	
22 L-Lever 		58 Sear Lifter Spring 	
23 R-Lever 		59 Sear Lifter Level Pin 	
24 Hinge 		60 Pin 	
25 Lever Spring 		61 Screw 	
26 Screw 		62 Trigger Plate 	
27 Receiver 		63 Screw 	
28 Cam 		64 Trigger Guard 	
30 Sear Pin 		65 Trigger Guard Screw 	
31 L-Sear 		66 R-Trigger 	
32 L-Hammer Assembly 		67 Trigger Spring 	
33 Plug 		68 L-Trigger 	
34 Plug Screw 		69 Pin 	
35 Follower 		70 Stock 	
36 L-Rod Assembly 
37 R-Rod Assembly 		71 Screw 	
38 Cocking Lever 		72 Washer 	
39 Cocking Lever Pin 		73 Butt Plate 	
40 Screw 		74 Woodscrew 
75 Woodscrew 	
41 Locking Lever 		77 Sear Spring 	
42 R-Hammer Assembly 		78 Wright	
 	 	79 Pin 	
 	 	80 Safety Spring 	
 	 	81 Bushing 	
			
Fig. #1		Fig. #3	
1a Receiver 		1c L-Sear 		
2a R-Trigger 		2c R-Sear 		
3a L-Trigger 		3c Trigger 		
4a L-Sear 		4c Spring 		
5a R-Sear 		5c Selector Plunger 		
6a Safety W/Cotter 		6c Selector 					
 							
Fig. #2							
1b Barrel Assembly 							
2b Exractor 							
3b Extractor Pin 							
4b Hinge 							
5b Follower 							
7b Receiver